{"status":"success","data":[{"id":5011,"name":"FreeRTOS","lib_id":440,"cn":"免费的RTOS","en":"FreeRTOS","jp":"","de":"Kostenloses RTOS","fr":"RTOS gratuit","es":"","ru":"","it":"RTOS gratuito","pt":"RTOS grátis","kr":"","tw":"","name_id":""},{"id":5012,"name":"AWS-IoT-_Device-Management","lib_id":440,"cn":"AWS物联网设备管理","en":"AWS-IoT-_Device-Management","jp":"","de":"AWS IoT-Geräteverwaltung","fr":"Gestion des appareils AWS IoT","es":"","ru":"","it":"Gestione dei dispositivi AWS IoT","pt":"Gerenciamento de dispositivo AWS IoT","kr":"","tw":"","name_id":""},{"id":5013,"name":"AWS-IoT-1-Click","lib_id":440,"cn":"AWS物联网1点击","en":"AWS-IoT-1-Click","jp":"","de":"AWS IoT 1 Klick","fr":"AWS IoT 1 clic","es":"","ru":"","it":"AWS IoT 1 clic","pt":"AWS IoT 1 clique","kr":"","tw":"","name_id":""},{"id":5014,"name":"AWS-IoT-Analytics","lib_id":440,"cn":"AWS物联网分析","en":"AWS-IoT-Analytics","jp":"","de":"AWS IoT-Analyse","fr":"Analyse AWS IoT","es":"","ru":"","it":"Analisi AWS IoT","pt":"Análise AWS IoT","kr":"","tw":"","name_id":""},{"id":5015,"name":"AWS-IoT-Button","lib_id":440,"cn":"AWS物联网按钮","en":"AWS-IoT-Button","jp":"","de":"AWS IoT-Schaltfläche","fr":"Bouton AWS IoT","es":"","ru":"","it":"Pulsante AWS IoT","pt":"Botão AWS IoT","kr":"","tw":"","name_id":""},{"id":5016,"name":"AWS-IoT-Core","lib_id":440,"cn":"AWS物联网核心","en":"AWS-IoT-Core","jp":"","de":"AWS IoT-Kern","fr":"Cœur AWS IoT","es":"","ru":"","it":"Core AWS IoT","pt":"Núcleo AWS IoT","kr":"","tw":"","name_id":""},{"id":5017,"name":"AWS-IoT-Device-Defender","lib_id":440,"cn":"AWS物联网设备防御者","en":"AWS-IoT-Device-Defender","jp":"","de":"AWS IoT Device Defender","fr":"AWS Défenseur des appareils IoT","es":"","ru":"","it":"AWS IoT Device Defender","pt":"Dispositivo de defesa AWS IoT","kr":"","tw":"","name_id":""},{"id":5018,"name":"AWS-IoT-Events","lib_id":440,"cn":"AWS物联网事件","en":"AWS-IoT-Events","jp":"","de":"AWS IoT-Ereignisse","fr":"Événements AWS IoT","es":"","ru":"","it":"Eventi AWS IoT","pt":"Eventos AWS IoT","kr":"","tw":"","name_id":""},{"id":5019,"name":"AWS-IoT-Greengrass","lib_id":440,"cn":"AWS物联网緑草","en":"AWS-IoT-Greengrass","jp":"","de":"AWS IoT Green Grass","fr":"Herbe verte AWS Monogatari","es":"","ru":"","it":"AWS IoT Greengrass","pt":"AWS Monogatari Green Grass","kr":"","tw":"","name_id":""},{"id":5020,"name":"AWS-IoT-SiteWise","lib_id":440,"cn":"AWS物联网网站明智","en":"AWS-IoT-SiteWise","jp":"","de":"AWS IoT-Website weise","fr":"Site Web AWS IoT sage","es":"","ru":"","it":"SiteWise AWS IoT","pt":"AWS IoT website wise","kr":"","tw":"","name_id":""},{"id":5021,"name":"AWS-IoT-Things-Graph","lib_id":440,"cn":"AWS物联网事物图","en":"AWS-IoT-Things-Graph","jp":"","de":"AWS IoT Things Diagramm","fr":"Diagramme d'objets AWS IoT","es":"","ru":"","it":"Diagramma AWS IoT Things","pt":"Diagrama de coisas a fazer da AWS IoT","kr":"","tw":"","name_id":""},{"id":5022,"name":"Internet-of-Things","lib_id":440,"cn":"物联网","en":"Internet-of-Things","jp":"","de":"Internet der Dinge","fr":"Internet des objets","es":"","ru":"","it":"Internet of Things","pt":"IoT","kr":"","tw":"","name_id":""},{"id":5023,"name":"AWS-IoT-Analytics_Pipeline","lib_id":440,"cn":"AWS物联网分析管道","en":"AWS-IoT-Analytics_Pipeline","jp":"","de":"AWS IoT-Analysepipeline","fr":"Pipeline d'analyse AWS IoT","es":"","ru":"","it":"Pipeline di analisi AWS IoT","pt":"Analise Pipeline AWS IoT","kr":"","tw":"","name_id":""},{"id":5024,"name":"AWS-IoT-Analytics_Data-Store","lib_id":440,"cn":"AWS物联网分析数据存储","en":"AWS-IoT-Analytics_Data-Store","jp":"","de":"AWS IoT-Analysedatenspeicher","fr":"Stockage des données d'analyse AWS IoT","es":"","ru":"","it":"Archiviazione dei dati dell'analisi AWS IoT","pt":"Armazenamento de dados de análise AWS IoT","kr":"","tw":"","name_id":""},{"id":5025,"name":"AWS-IoT-Analytics_Data-Set","lib_id":440,"cn":"AWS物联网分析数据集","en":"AWS-IoT-Analytics_Data-Set","jp":"","de":"AWS IoT-Analysedatensatz","fr":"Ensemble de données d'analyse AWS IoT","es":"","ru":"","it":"Set di dati di analisi AWS IoT","pt":"Conjunto de dados de análise AWS IoT","kr":"","tw":"","name_id":""},{"id":5026,"name":"AWS-IoT-Analytics_Channel","lib_id":440,"cn":"AWS物联网分析渠道","en":"AWS-IoT-Analytics_Channel","jp":"","de":"AWS IoT-Analysekanäle","fr":"Canaux d'analyse AWS IoT","es":"","ru":"","it":"Canali di analisi AWS IoT","pt":"Canais de análise AWS IoT","kr":"","tw":"","name_id":""},{"id":5027,"name":"AWS-IoT-Analytics_Notebook","lib_id":440,"cn":"AWS物联网分析笔记本","en":"AWS-IoT-Analytics_Notebook","jp":"","de":"AWS-IoT-Analytics-Notizbuch","fr":"Bloc-notes AWS-IoT-Analytics","es":"","ru":"","it":"Notebook di analisi AWS IoT","pt":"Bloco de notas analítico AWS IoT","kr":"","tw":"","name_id":""},{"id":5028,"name":"AWS-IoT-Greengrass_Connector","lib_id":440,"cn":"AWS物联网Greengrass连接器","en":"AWS-IoT-Greengrass_Connector","jp":"","de":"AWS IoT Greengrass Connector","fr":"Connecteur AWS IoT Greengrass","es":"","ru":"","it":"Connettore AWS IoT Greengrass","pt":"Conector AWS IoT Greengrass","kr":"","tw":"","name_id":""},{"id":5029,"name":"IoT_Action","lib_id":440,"cn":"物联网行动","en":"IoT_Action","jp":"","de":"IoT-Aktion","fr":"Action IoT","es":"","ru":"","it":"Azione IoT","pt":"Ação IoT","kr":"","tw":"","name_id":""},{"id":5030,"name":"IoT_Actuator","lib_id":440,"cn":"物联网执行器","en":"IoT_Actuator","jp":"","de":"Aktuator für das Internet der Dinge","fr":"Actionneur Internet des objets","es":"","ru":"","it":"Attuatore Internet of Things","pt":"Atuador do IoT","kr":"","tw":"","name_id":""},{"id":5031,"name":"IoT_Alexa-enabled-device","lib_id":440,"cn":"物联网支持Alexa的设备","en":"IoT_Alexa-enabled-device","jp":"","de":"IoT-Geräte, die Alexa unterstützen","fr":"Appareils IoT prenant en charge Alexa","es":"","ru":"","it":"Dispositivi IoT supporto Alexa","pt":"Dispositivos IoT compatíveis com Alexa","kr":"","tw":"","name_id":""},{"id":5032,"name":"IoT_Alexa-skill","lib_id":440,"cn":"物联网Alexa-技能","en":"IoT_Alexa-skill","jp":"","de":"IoT Alexa-Fähigkeiten","fr":"Compétences Alexa IoT","es":"","ru":"","it":"IoT Alexa-Skills","pt":"IoT Alexa-Skills","kr":"","tw":"","name_id":""},{"id":5033,"name":"IoT_Alexa-voice-service","lib_id":440,"cn":"物联网Alexa-语音服务","en":"IoT_Alexa-voice-service","jp":"","de":"Internet der Dinge Alexa-Voice Service","fr":"Service Alexa-Voice de l'Internet des objets","es":"","ru":"","it":"Internet of Things Servizio vocale Alexa","pt":"Serviço de vozes da Alexa IoT","kr":"","tw":"","name_id":""},{"id":5034,"name":"IoT_Bank","lib_id":440,"cn":"物联网银行","en":"IoT_Bank","jp":"","de":"Internet der Dinge Bank","fr":"Banque de l'Internet des objets","es":"","ru":"","it":"Banca Internet delle cose","pt":"Banco IoT","kr":"","tw":"","name_id":""},{"id":5035,"name":"IoT_Bicycle","lib_id":440,"cn":"物联网自行车","en":"IoT_Bicycle","jp":"","de":"Internet der Dinge Fahrrad","fr":"Vélo Internet des objets","es":"","ru":"","it":"Internet of Things Bike","pt":"Bicicleta - IoT","kr":"","tw":"","name_id":""},{"id":5036,"name":"IoT_Camera","lib_id":440,"cn":"物联网相机","en":"IoT_Camera","jp":"","de":"IoT-Kamera ","fr":"Caméra IoT","es":"","ru":"","it":"Fotocamera IoT","pt":"Câmera IoT","kr":"","tw":"","name_id":""},{"id":5037,"name":"IoT_Car","lib_id":440,"cn":"物联网汽车","en":"IoT_Car","jp":"","de":"IoT Auto","fr":"Voiture IoT","es":"","ru":"","it":"Auto IoT","pt":"Carro IoT","kr":"","tw":"","name_id":""},{"id":5038,"name":"IoT_Cart","lib_id":440,"cn":"物联网购物车","en":"IoT_Cart","jp":"","de":"IoT Einkaufswagen","fr":"Panier IoT","es":"","ru":"","it":"Carrello della spesa IoT","pt":"IoT carrinho de compras","kr":"","tw":"","name_id":""},{"id":5039,"name":"IoT_Certificate-manager","lib_id":440,"cn":"物联网证书管理器","en":"IoT_Certificate-manager","jp":"","de":"IoT-Zertifikatmanager","fr":"Gestionnaire de certificats IoT","es":"","ru":"","it":"Gestore dei certificati IoT","pt":"Gerenciador de certificado IoT","kr":"","tw":"","name_id":""},{"id":5040,"name":"IoT_Coffee-pot","lib_id":440,"cn":"物联网咖啡壶","en":"IoT_Coffee-pot","jp":"","de":"IoT-Zertifikatmanager","fr":"Cafetière Internet des objets","es":"","ru":"","it":"Internet delle cose macchina per il caffè","pt":"Pote de café IoT","kr":"","tw":"","name_id":""},{"id":5041,"name":"IoT_Desired-state","lib_id":440,"cn":"物联网所需状态","en":"IoT_Desired-state","jp":"","de":"Der erforderliche Zustand des Internet der Dinge","fr":"L'état requis de l'Internet des objets","es":"","ru":"","it":"Lo stato richiesto dell'Internet of Things","pt":"Estado desejado IoT\"","kr":"","tw":"","name_id":""},{"id":5042,"name":"IoT_Device-gateway","lib_id":440,"cn":"物联网设备网关","en":"IoT_Device-gateway","jp":"","de":"IoT-Geräte-Gateway","fr":"Passerelle d'appareils IoT","es":"","ru":"","it":"Gateway del dispositivo IoT","pt":"Gateway de dispositivo IoT","kr":"","tw":"","name_id":""},{"id":5043,"name":"IoT_Door-lock","lib_id":440,"cn":"物联网门锁","en":"IoT_Door-lock","jp":"","de":"IoT Türschloss","fr":"Serrure de porte IoT","es":"","ru":"","it":"Serratura della porta IoT","pt":"Fechadura de porta IoT","kr":"","tw":"","name_id":""},{"id":5044,"name":"IoT_Echo","lib_id":440,"cn":"物联网回声","en":"IoT_Echo","jp":"","de":"IoT-Echo","fr":"Écho IoT","es":"","ru":"","it":"IoT Echo","pt":"IoT echo","kr":"","tw":"","name_id":""},{"id":5045,"name":"IoT_Factory","lib_id":440,"cn":"物联网工厂","en":"IoT_Factory","jp":"","de":"IoT-Fabrik","fr":"Usine IoT","es":"","ru":"","it":"Fabbrica IoT","pt":"Fábrica de IoT","kr":"","tw":"","name_id":""},{"id":5046,"name":"IoT_Fire-TV","lib_id":440,"cn":"物联网消防电视","en":"IoT_Fire-TV","jp":"","de":"IoT Fire TV","fr":"IoT Fire TV","es":"","ru":"","it":"IoT Fire TV","pt":"IoT Fire TV","kr":"","tw":"","name_id":""},{"id":5047,"name":"IoT_Fire-TV-stick","lib_id":440,"cn":"物联网消防电视棒","en":"IoT_Fire-TV-stick","jp":"","de":"IoT Fire TV Stick","fr":"Clé TV IoT Fire","es":"","ru":"","it":"IoT Fire TV Stick","pt":"IoT Fire TV Stick","kr":"","tw":"","name_id":""},{"id":5048,"name":"IoT_Generic","lib_id":440,"cn":"通用物联网","en":"IoT_Generic","jp":"","de":"Allgemeines Internet der Dinge","fr":"Internet des objets général","es":"","ru":"","it":"Internet delle cose generale","pt":"Genérico IoT","kr":"","tw":"","name_id":""},{"id":5049,"name":"IoT_Hardware-board","lib_id":440,"cn":"物联网硬件板","en":"IoT_Hardware-board","jp":"","de":"IoT-Hardware-Karte","fr":"Carte matérielle IoT","es":"","ru":"","it":"Scheda hardware IoT","pt":"Placa de hardware IoT","kr":"","tw":"","name_id":""},{"id":5050,"name":"IoT_House","lib_id":440,"cn":"物联网之家","en":"IoT_House","jp":"","de":"Heimat des Internet der Dinge","fr":"Accueil de l'Internet des objets","es":"","ru":"","it":"Home of the Internet of Things","pt":"Casa IoT","kr":"","tw":"","name_id":""},{"id":5051,"name":"IoT_HTTP-2-protocol","lib_id":440,"cn":"物联网HTTP-2协议","en":"IoT_HTTP-2-protocol","jp":"","de":"Internet of Things HTTP-2-Protokoll","fr":"Protocole Internet des objets HTTP-2","es":"","ru":"","it":"Protocollo HTTP-2 di Internet of Things","pt":"Protocolo HTTP-2 da IoT","kr":"","tw":"","name_id":""},{"id":5052,"name":"IoT_HTTP-protocol","lib_id":440,"cn":"物联网HTTP协议","en":"IoT_HTTP-protocol","jp":"","de":"HTTP-Protokoll für das Internet der Dinge","fr":"Protocole HTTP de l'Internet des objets","es":"","ru":"","it":"Protocollo HTTP Internet of Things","pt":"Protocolo HTTP da IoT","kr":"","tw":"","name_id":""},{"id":5053,"name":"IoT_Lambda-function","lib_id":440,"cn":"物联网Lambda功能","en":"IoT_Lambda-function","jp":"","de":"IoT Lambda-Funktion","fr":"Fonction IoT Lambda","es":"","ru":"","it":"Funzione Lambda IoT","pt":"Função IoT Lambda","kr":"","tw":"","name_id":""},{"id":5054,"name":"IoT_Lightbulb","lib_id":440,"cn":"物联网灯泡","en":"IoT_Lightbulb","jp":"","de":"IoT Glühbirne","fr":"Ampoule IoT","es":"","ru":"","it":"Lampadina IoT","pt":"Lâmpada IoT","kr":"","tw":"","name_id":""},{"id":5055,"name":"IoT_Medical-emergency","lib_id":440,"cn":"物联网医疗急救","en":"IoT_Medical-emergency","jp":"","de":"IoT Glühbirne","fr":"Urgence médicale IoT","es":"","ru":"","it":"Emergenza medica IoT","pt":"Emergência médica IoT","kr":"","tw":"","name_id":""},{"id":5056,"name":"IoT_MQTT-protocol","lib_id":440,"cn":"物联网MQTT协议","en":"IoT_MQTT-protocol","jp":"","de":"IoT MQTT-Protokoll","fr":"Protocole IoT MQTT","es":"","ru":"","it":"Protocollo IoT MQTT","pt":"Protocolo IoT MQTT","kr":"","tw":"","name_id":""},{"id":5057,"name":"IoT_Over-the-air-update","lib_id":440,"cn":"物联网空中更新","en":"IoT_Over-the-air-update","jp":"","de":"Internet der Dinge Update","fr":"Mise à jour de l'Internet des objets","es":"","ru":"","it":"Aggiornamento Internet of Things","pt":"Atualização da IoT","kr":"","tw":"","name_id":""},{"id":5058,"name":"IoT_Police-emergency","lib_id":440,"cn":"物联网警察紧急情况","en":"IoT_Police-emergency","jp":"","de":"IoT Polizei Notfall","fr":"Urgence de la police IoT","es":"","ru":"","it":"Emergenza polizia IoT","pt":"Emergência policial IoT","kr":"","tw":"","name_id":""},{"id":5059,"name":"IoT_Policy","lib_id":440,"cn":"物联网政策","en":"IoT_Policy","jp":"","de":"IoT-Richtlinie","fr":"Politique IoT","es":"","ru":"","it":"Politica IoT","pt":"Política de IoT","kr":"","tw":"","name_id":""},{"id":5060,"name":"IoT_Reported-state","lib_id":440,"cn":"物联网报告状态","en":"IoT_Reported-state","jp":"","de":"IoT-Berichtsstatus","fr":"Politique IoT","es":"","ru":"","it":"Stato del report IoT","pt":"Status do relatório de IoT","kr":"","tw":"","name_id":""},{"id":5061,"name":"IoT_Rule","lib_id":440,"cn":"物联网规则","en":"IoT_Rule","jp":"","de":"Regeln für das Internet der Dinge","fr":"Règles de l'Internet des objets","es":"","ru":"","it":"Regole dell'Internet of Things","pt":"Regras da IoT","kr":"","tw":"","name_id":""},{"id":5062,"name":"IoT_Sensor","lib_id":440,"cn":"物联网传感器","en":"IoT_Sensor","jp":"","de":"IoT-Sensoren","fr":"Capteurs IoT","es":"","ru":"","it":"Sensori IoT","pt":"Sensores IoT","kr":"","tw":"","name_id":""},{"id":5063,"name":"IoT_Servo","lib_id":440,"cn":"物联网服务","en":"IoT_Servo","jp":"","de":"Internet der Dinge Service","fr":"Service Internet des objets","es":"","ru":"","it":"Servizio Internet of Things","pt":"Servo de IoT","kr":"","tw":"","name_id":""},{"id":5064,"name":"IoT_Shadow","lib_id":440,"cn":"物联网影子","en":"IoT_Shadow","jp":"","de":"Schatten des Internet der Dinge","fr":"Ombre de l'Internet des objets","es":"","ru":"","it":"Shadow IoT\t","pt":"IoT Shadow","kr":"","tw":"","name_id":""},{"id":5065,"name":"IoT_Simulator","lib_id":440,"cn":"物联网模拟器","en":"IoT_Simulator","jp":"","de":"IoT-Simulator","fr":"Simulateur IoT","es":"","ru":"","it":"Simulatore IoT","pt":"Simulador de IoT","kr":"","tw":"","name_id":""},{"id":5066,"name":"IoT_Thermostat","lib_id":440,"cn":"物联网恒温器","en":"IoT_Thermostat","jp":"","de":"IoT-Thermostat","fr":"Thermostat IoT","es":"","ru":"","it":"Termostato IoT","pt":"Termostato IoT","kr":"","tw":"","name_id":""},{"id":5067,"name":"IoT_Topic","lib_id":440,"cn":"物联网主题","en":"IoT_Topic","jp":"","de":"IoT-Thema","fr":"Thème IoT","es":"","ru":"","it":"Argomento IoT","pt":"Tópico IoT","kr":"","tw":"","name_id":""},{"id":5068,"name":"IoT_Travel","lib_id":440,"cn":"物联网旅行","en":"IoT_Travel","jp":"","de":"IoT Reisen","fr":"Voyage IoT","es":"","ru":"","it":"Viaggio IoT","pt":"Viagem IoT","kr":"","tw":"","name_id":""},{"id":5069,"name":"IoT_Utility","lib_id":440,"cn":"物联网实用程序","en":"IoT_Utility","jp":"","de":"IoT-Dienstprogramm","fr":"Utilitaire IoT","es":"","ru":"","it":"Utility IoT","pt":"Utilitário IoT","kr":"","tw":"","name_id":""},{"id":5070,"name":"IoT_Windfarm","lib_id":440,"cn":"物联网风电场","en":"IoT_Windfarm","jp":"","de":"IoT Windpark","fr":"Parc éolien IoT","es":"","ru":"","it":"Per centrali eoliche IoT","pt":"IoT Windfarm","kr":"","tw":"","name_id":""},{"id":5071,"name":"IoT-Device-Jobs_Resource","lib_id":440,"cn":"物联网设备作业资源","en":"IoT-Device-Jobs_Resource","jp":"","de":"Ressourcen für den Betrieb von IoT-Geräten","fr":"Ressources d'exploitation des appareils IoT","es":"","ru":"","it":"Risorsa lavori dispositivo IoT","pt":"Recurso de trabalhos da IoT","kr":"","tw":"","name_id":""}],"msg":""}