{"status":"success","data":[{"id":11197,"name":"Sensor of the measured non - electrical quantity","lib_id":521,"cn":"Sensor of the measured non - electrical quantity","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11198,"name":"Electrical measuring instrument Indicating","lib_id":521,"cn":"Electrical measuring instrument Indicating","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11199,"name":"Electrical measuring instrument Recording","lib_id":521,"cn":"Electrical measuring instrument Recording","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11200,"name":"Electrical measuring instrument Integrating","lib_id":521,"cn":"Electrical measuring instrument Integrating","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11201,"name":"Instrument, the movable part of which can deviate in one direction from the zero mark: to the right","lib_id":521,"cn":"Instrument, the movable part of which can deviate in one direction from the zero mark: to the right","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11202,"name":"Instrument, the movable part of which can deviate in one direction from the zero mark: to the left","lib_id":521,"cn":"Instrument, the movable part of which can deviate in one direction from the zero mark: to the left","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11203,"name":"прибор вибрационной системы","lib_id":521,"cn":"прибор вибрационной системы","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11204,"name":"Vibrating system instrument","lib_id":521,"cn":"Vibrating system instrument","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11205,"name":"Instrument with digital reading","lib_id":521,"cn":"Instrument with digital reading","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11206,"name":"Instrument with continuous recording (recording)","lib_id":521,"cn":"Instrument with continuous recording (recording)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11207,"name":"Instrument with dot recording (recording)","lib_id":521,"cn":"Instrument with dot recording (recording)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11208,"name":"Printing instrument with digital recording","lib_id":521,"cn":"Printing instrument with digital recording","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11209,"name":"Instrument with perforation recording","lib_id":521,"cn":"Instrument with perforation recording","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11210,"name":"Galvanometer","lib_id":521,"cn":"Galvanometer","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11211,"name":"Synchroscope","lib_id":521,"cn":"Synchroscope","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11212,"name":"Oscilloscope","lib_id":521,"cn":"Oscilloscope","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11213,"name":"Oscillograph","lib_id":521,"cn":"Oscillograph","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11214,"name":"Oscillographic galvanometer:of current or voltage","lib_id":521,"cn":"Oscillographic galvanometer:of current or voltage","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11215,"name":"Oscillographic galvanometer:of instantaneous power","lib_id":521,"cn":"Oscillographic galvanometer:of instantaneous power","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11216,"name":"Pulse counter","lib_id":521,"cn":"Pulse counter","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11217,"name":"Electrometer","lib_id":521,"cn":"Electrometer","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11218,"name":"Semiconductor bolometer","lib_id":521,"cn":"Semiconductor bolometer","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11219,"name":"Temperature sensor","lib_id":521,"cn":"Temperature sensor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11220,"name":"Pressure sensor","lib_id":521,"cn":"Pressure sensor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11221,"name":"Secondary clocks","lib_id":521,"cn":"Secondary clocks","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11222,"name":"Primary clocks","lib_id":521,"cn":"Primary clocks","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11223,"name":"Clocks with contact device","lib_id":521,"cn":"Clocks with contact device","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11224,"name":"Synchronous clocks","lib_id":521,"cn":"Synchronous clocks","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11225,"name":"Indicator of maximum active power with feedback to a wattmeter","lib_id":521,"cn":"Indicator of maximum active power with feedback to a wattmeter","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11226,"name":"Differential voltmeter","lib_id":521,"cn":"Differential voltmeter","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11227,"name":"Salinometer","lib_id":521,"cn":"Salinometer","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11228,"name":"Self - recording combined wattmeter and varmeter","lib_id":521,"cn":"Self - recording combined wattmeter and varmeter","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11229,"name":"Time counter","lib_id":521,"cn":"Time counter","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11230,"name":"Watt - hour meter for measuring energy transferred in one direction","lib_id":521,"cn":"Watt - hour meter for measuring energy transferred in one direction","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11231,"name":"Watt - hour meter with maximum active power registration","lib_id":521,"cn":"Watt - hour meter with maximum active power registration","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11232,"name":"Distinctive symbol of the event counting function","lib_id":521,"cn":"Distinctive symbol of the event counting function","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11233,"name":"Electric pulse counter with manual setting to n (set to zero when n = 0)","lib_id":521,"cn":"Electric pulse counter with manual setting to n (set to zero when n = 0)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11234,"name":"Electric pulse counter with electrical zero setting","lib_id":521,"cn":"Electric pulse counter with electrical zero setting","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11235,"name":"Electric pulse counter with multiple contacts","lib_id":521,"cn":"Electric pulse counter with multiple contacts","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11236,"name":"Counting device controlled by a cam and controlling the closing of a contact every n events","lib_id":521,"cn":"Counting device controlled by a cam and controlling the closing of a contact every n events","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""}],"msg":""}