{"status":"success","data":[{"id":11172,"name":"Armature of electromechanical device. General symbol","lib_id":520,"cn":"Armature of electromechanical device. General symbol","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11173,"name":"Armature of electromechanical device with one winding","lib_id":520,"cn":"Armature of electromechanical device with one winding","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11174,"name":"Armature of electromechanical device with two windings","lib_id":520,"cn":"Armature of electromechanical device with two windings","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11175,"name":"Armature of electromechanical device with n windings","lib_id":520,"cn":"Armature of electromechanical device with n windings","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11176,"name":"Coil of an electromechanical device with two opposing windings","lib_id":520,"cn":"Coil of an electromechanical device with two opposing windings","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11177,"name":"Coil of an electromechanical device with two identical opposing windings (bifilar winding)","lib_id":520,"cn":"Coil of an electromechanical device with two identical opposing windings (bifilar winding)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11178,"name":"Coil of an electromechanical device with one lead - out","lib_id":520,"cn":"Coil of an electromechanical device with one lead - out","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11179,"name":"Coil of an electromechanical device for three-phase current","lib_id":520,"cn":"Coil of an electromechanical device for three-phase current","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11180,"name":"Coil of an electromechanical device with an additional graphical field:with one additional graphical field","lib_id":520,"cn":"Coil of an electromechanical device with an additional graphical field:with one additional graphical field","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11181,"name":"Coil of an electromechanical device with an additional graphical field:with two additional graphical fields","lib_id":520,"cn":"Coil of an electromechanical device with an additional graphical field:with two additional graphical fields","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11182,"name":"Coil of an electromechanical device with indication of the type of winding:current winding","lib_id":520,"cn":"Coil of an electromechanical device with indication of the type of winding:current winding","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11183,"name":"Coil of an electromechanical device with indication of the type of winding:Voltage winding","lib_id":520,"cn":"Coil of an electromechanical device with indication of the type of winding:Voltage winding","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11184,"name":"Coil of an electromechanical device with indication of the type of winding:Maximum - current winding","lib_id":520,"cn":"Coil of an electromechanical device with indication of the type of winding:Maximum - current winding","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11185,"name":"Coil of an electromechanical device with indication of the type of winding:Minimum - voltage winding","lib_id":520,"cn":"Coil of an electromechanical device with indication of the type of winding:Minimum - voltage winding","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11186,"name":"Coil of a polarized electromechanical device","lib_id":520,"cn":"Coil of a polarized electromechanical device","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11187,"name":"Coil of an electromechanical device with residual magnetism","lib_id":520,"cn":"Coil of an electromechanical device with residual magnetism","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11188,"name":"Coil of an electromechanical device with a mechanical lock","lib_id":520,"cn":"Coil of an electromechanical device with a mechanical lock","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11189,"name":"Coil of an electromechanical device that accelerates during actuation","lib_id":520,"cn":"Coil of an electromechanical device that accelerates during actuation","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11190,"name":"Coil of an electromechanical device that accelerates during actuation and release","lib_id":520,"cn":"Coil of an electromechanical device that accelerates during actuation and release","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11191,"name":"Coil of an electromechanical device that decelerates during actuation","lib_id":520,"cn":"Coil of an electromechanical device that decelerates during actuation","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11192,"name":"Coil of an electromechanical device that decelerates during release","lib_id":520,"cn":"Coil of an electromechanical device that decelerates during release","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11193,"name":"Coil of an electromechanical device that decelerates during actuation and release","lib_id":520,"cn":"Coil of an electromechanical device that decelerates during actuation and release","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11194,"name":"Coil of an electromechanical device insensitive to alternating current","lib_id":520,"cn":"Coil of an electromechanical device insensitive to alternating current","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11195,"name":"Coil of an electromechanical device operating in a state of mechanical resonance","lib_id":520,"cn":"Coil of an electromechanical device operating in a state of mechanical resonance","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11196,"name":"Sensing part of the electro - thermal relay","lib_id":520,"cn":"Sensing part of the electro - thermal relay","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""}],"msg":""}