{"status":"success","data":[{"id":11286,"name":"Electrodes: base with one lead","lib_id":524,"cn":"Electrodes: base with one lead","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11287,"name":"Electrodes: Base with two leads","lib_id":524,"cn":"Electrodes: Base with two leads","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11288,"name":"Electrodes: P-emitter with N-region","lib_id":524,"cn":"Electrodes: P-emitter with N-region","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11289,"name":"Electrodes: N-emitter with P-region","lib_id":524,"cn":"Electrodes: N-emitter with P-region","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11290,"name":"Electrodes: Multiple P-emitters with N-region","lib_id":524,"cn":"Electrodes: Multiple P-emitters with N-region","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11291,"name":"Electrodes: Multiple N-emitters with P-region","lib_id":524,"cn":"Electrodes: Multiple N-emitters with P-region","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11292,"name":"Electrodes: Collector with base","lib_id":524,"cn":"Electrodes: Collector with base","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11293,"name":"Electrodes: Multiple collectors (e.g., four collectors on base)","lib_id":524,"cn":"Electrodes: Multiple collectors (e.g., four collectors on base)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11294,"name":"Regions: Region between conductive layers with different conductivity","lib_id":524,"cn":"Regions: Region between conductive layers with different conductivity","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11295,"name":"Regions: between regions with different types of conductivity (PIN or NIP)","lib_id":524,"cn":"Regions: between regions with different types of conductivity (PIN or NIP)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11296,"name":"Regions: between regions with the same type of conductivity (PIP or NIN)","lib_id":524,"cn":"Regions: between regions with the same type of conductivity (PIP or NIN)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11297,"name":"Regions: between the collector and a region with opposite conductivity (PIN or NIP)","lib_id":524,"cn":"Regions: between the collector and a region with opposite conductivity (PIN or NIP)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11298,"name":"Regions: between the collector and a region with the same type of conductivity (PIP or NIN)","lib_id":524,"cn":"Regions: between the collector and a region with the same type of conductivity (PIP or NIN)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11299,"name":"Conduction channel for field-effect transistors: enhancement type","lib_id":524,"cn":"Conduction channel for field-effect transistors: enhancement type","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11300,"name":"Conduction channel for field-effect transistors: depletion type","lib_id":524,"cn":"Conduction channel for field-effect transistors: depletion type","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11301,"name":"PN junction","lib_id":524,"cn":"PN junction","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11302,"name":"NP junction","lib_id":524,"cn":"NP junction","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11303,"name":"P-channel on N-substrate (enhancement)","lib_id":524,"cn":"P-channel on N-substrate (enhancement)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11304,"name":"N-channel on P-substrate (enhancement)","lib_id":524,"cn":"N-channel on P-substrate (enhancement)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11305,"name":"Insulated gate","lib_id":524,"cn":"Insulated gate","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11306,"name":"Source and drain","lib_id":524,"cn":"Source and drain","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11307,"name":"Leads of semiconductor devices: electrically not connected to the housing","lib_id":524,"cn":"Leads of semiconductor devices: electrically not connected to the housing","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11308,"name":"Leads of semiconductor devices: electrically connected to the housing","lib_id":524,"cn":"Leads of semiconductor devices: electrically connected to the housing","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11309,"name":"External body lead. It is permissible to change the dot at the point of attachment to the body","lib_id":524,"cn":"External body lead. It is permissible to change the dot at the point of attachment to the body","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11310,"name":"Tunnel effect (direct)","lib_id":524,"cn":"Tunnel effect (direct)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11311,"name":"Tunnel effect (reverse)","lib_id":524,"cn":"Tunnel effect (reverse)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11312,"name":"Avalanche breakdown (unidirectional)","lib_id":524,"cn":"Avalanche breakdown (unidirectional)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11313,"name":"Avalanche breakdown (bidirectional)","lib_id":524,"cn":"Avalanche breakdown (bidirectional)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11314,"name":"Schottky effect","lib_id":524,"cn":"Schottky effect","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11315,"name":"Diode (general)","lib_id":524,"cn":"Diode (general)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11316,"name":"Tunnel diode","lib_id":524,"cn":"Tunnel diode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11317,"name":"Reverse diode","lib_id":524,"cn":"Reverse diode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11318,"name":"Zener diode (avalanche rectifier diode): unidirectional","lib_id":524,"cn":"Zener diode (avalanche rectifier diode): unidirectional","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11319,"name":"Zener diode (avalanche rectifier diode): bidirectional","lib_id":524,"cn":"Zener diode (avalanche rectifier diode): bidirectional","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11320,"name":"Thermoelectric diode","lib_id":524,"cn":"Thermoelectric diode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11321,"name":"Varicap (capacitive diode)","lib_id":524,"cn":"Varicap (capacitive diode)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11322,"name":"Bidirectional diode","lib_id":524,"cn":"Bidirectional diode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11323,"name":"Module with multiple (for example, three) identical diodes with a common anode and separate cathode outputs","lib_id":524,"cn":"Module with multiple (for example, three) identical diodes with a common anode and separate cathode outputs","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11324,"name":"Module with multiple identical diodes with a common cathode and separate anode outputs","lib_id":524,"cn":"Module with multiple identical diodes with a common cathode and separate anode outputs","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11325,"name":"Schottky diode","lib_id":524,"cn":"Schottky diode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11326,"name":"Light-emitting diode (LED)","lib_id":524,"cn":"Light-emitting diode (LED)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11327,"name":"Reverse-blocking diode thyristor","lib_id":524,"cn":"Reverse-blocking diode thyristor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11328,"name":"Reverse-conducting diode thyristor","lib_id":524,"cn":"Reverse-conducting diode thyristor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11329,"name":"Symmetrical diode thyristor","lib_id":524,"cn":"Symmetrical diode thyristor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11330,"name":"Triode thyristor. General symbol","lib_id":524,"cn":"Triode thyristor. General symbol","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11331,"name":"Reverse-blocking triode thyristor：anode","lib_id":524,"cn":"Reverse-blocking triode thyristor：anode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11332,"name":"Reverse-blocking triode thyristor：cathode","lib_id":524,"cn":"Reverse-blocking triode thyristor：cathode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11333,"name":"Turn-off triode thyristor: general symbol","lib_id":524,"cn":"Turn-off triode thyristor: general symbol","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11334,"name":"Turn-off triode thyristor: reverse-blocking, with anode control","lib_id":524,"cn":"Turn-off triode thyristor: reverse-blocking, with anode control","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11335,"name":"Turn-off triode thyristor: reverse-blocking, with cathode control","lib_id":524,"cn":"Turn-off triode thyristor: reverse-blocking, with cathode control","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11336,"name":"Reverse-conducting triode thyristor: general symbol","lib_id":524,"cn":"Reverse-conducting triode thyristor: general symbol","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11337,"name":"Reverse-conducting triode thyristor: with anode control","lib_id":524,"cn":"Reverse-conducting triode thyristor: with anode control","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11338,"name":"Reverse-conducting triode thyristor: with cathode control","lib_id":524,"cn":"Reverse-conducting triode thyristor: with cathode control","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11339,"name":"Bidirectional triode thyristor (TRIAC)","lib_id":524,"cn":"Bidirectional triode thyristor (TRIAC)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11340,"name":"Reverse-blocking tetrode thyristor","lib_id":524,"cn":"Reverse-blocking tetrode thyristor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11341,"name":"PNP transistor","lib_id":524,"cn":"PNP transistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11342,"name":"NPN transistor (with internal screen)","lib_id":524,"cn":"NPN transistor (with internal screen)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11343,"name":"NPN transistor (collector connected to case)","lib_id":524,"cn":"NPN transistor (collector connected to case)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11344,"name":"Avalanche NPN transistor","lib_id":524,"cn":"Avalanche NPN transistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11345,"name":"Unijunction transistor (N-base)","lib_id":524,"cn":"Unijunction transistor (N-base)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11346,"name":"Unijunction transistor (P-base)","lib_id":524,"cn":"Unijunction transistor (P-base)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11347,"name":"Dual-base NPN transistor","lib_id":524,"cn":"Dual-base NPN transistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11348,"name":"PNIP dual-base transistor (I-region lead)","lib_id":524,"cn":"PNIP dual-base transistor (I-region lead)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11349,"name":"Multi-emitter NPN transistor","lib_id":524,"cn":"Multi-emitter NPN transistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11350,"name":"The following is permitted when creating diagrams:represent transistor symbols in mirror image","lib_id":524,"cn":"The following is permitted when creating diagrams:represent transistor symbols in mirror image","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11351,"name":"FET with N-channel","lib_id":524,"cn":"FET with N-channel","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11352,"name":"FET with P-channel","lib_id":524,"cn":"FET with P-channel","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11353,"name":"P-channel Enhancement-mode MOSFET (with no substrate terminal)","lib_id":524,"cn":"P-channel Enhancement-mode MOSFET (with no substrate terminal)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11354,"name":"N-channel Enhancement-mode MOSFET (with no substrate terminal)","lib_id":524,"cn":"N-channel Enhancement-mode MOSFET (with no substrate terminal)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11355,"name":"P-channel Depletion-mode MOSFET (with no substrate terminal)","lib_id":524,"cn":"P-channel Depletion-mode MOSFET (with no substrate terminal)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11356,"name":"N-channel Depletion-mode MOSFET (with no substrate terminal)","lib_id":524,"cn":"N-channel Depletion-mode MOSFET (with no substrate terminal)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11357,"name":"MOSFET (N-channel, source-substrate connected)","lib_id":524,"cn":"MOSFET (N-channel, source-substrate connected)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11358,"name":"MOSFET (P-channel, substrate lead)","lib_id":524,"cn":"MOSFET (P-channel, substrate lead)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11359,"name":"Dual-gate MOSFET (P-channel)","lib_id":524,"cn":"Dual-gate MOSFET (P-channel)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11360,"name":"FET with Schottky gate","lib_id":524,"cn":"FET with Schottky gate","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11361,"name":"Dual Schottky-gate FET","lib_id":524,"cn":"Dual Schottky-gate FET","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11362,"name":"Photoresistor (general)","lib_id":524,"cn":"Photoresistor (general)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11363,"name":"Differential photoresistor","lib_id":524,"cn":"Differential photoresistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11364,"name":"Photodiode","lib_id":524,"cn":"Photodiode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11365,"name":"Photothyristor","lib_id":524,"cn":"Photothyristor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11366,"name":"Phototransistor (PNP)","lib_id":524,"cn":"Phototransistor (PNP)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11367,"name":"Phototransistor (NPN)","lib_id":524,"cn":"Phototransistor (NPN)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11368,"name":"Photocell","lib_id":524,"cn":"Photocell","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11369,"name":"Photovoltaic array","lib_id":524,"cn":"Photovoltaic array","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11370,"name":"Diode optocoupler","lib_id":524,"cn":"Diode optocoupler","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11371,"name":"Thyristor optocoupler","lib_id":524,"cn":"Thyristor optocoupler","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11372,"name":"Resistor optocoupler","lib_id":524,"cn":"Resistor optocoupler","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11373,"name":"Optoelectronic device with photodiode and amplifier: integrated","lib_id":524,"cn":"Optoelectronic device with photodiode and amplifier: integrated","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11374,"name":"Optoelectronic device with photodiode and amplifier: separated","lib_id":524,"cn":"Optoelectronic device with photodiode and amplifier: separated","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11375,"name":"Optoelectronic device with phototransistor: with base lead","lib_id":524,"cn":"Optoelectronic device with phototransistor: with base lead","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11376,"name":"Optoelectronic device with phototransistor: without base lead","lib_id":524,"cn":"Optoelectronic device with phototransistor: without base lead","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11377,"name":"Optoelectronic devices: It is permitted to depict optoelectronic devices in a separated manner","lib_id":524,"cn":"Optoelectronic devices: It is permitted to depict optoelectronic devices in a separated manner","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11378,"name":"Optoelectronic devices: The mutual orientation of the source and receiver symbols is not fixed and is determined by the convenience of drawing the diagram","lib_id":524,"cn":"Optoelectronic devices: The mutual orientation of the source and receiver symbols is not fixed and is determined by the convenience of drawing the diagram","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11379,"name":"Hall sensor","lib_id":524,"cn":"Hall sensor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11380,"name":"Magneto-resistor","lib_id":524,"cn":"Magneto-resistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11381,"name":"Magnetic splitter","lib_id":524,"cn":"Magnetic splitter","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11382,"name":"Single-phase bridge rectifier (expanded)","lib_id":524,"cn":"Single-phase bridge rectifier (expanded)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11383,"name":"Single-phase bridge rectifier (simplified)","lib_id":524,"cn":"Single-phase bridge rectifier (simplified)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11384,"name":"Single-phase bridge rectifier: Example of the application of the graphical symbol in a diagram","lib_id":524,"cn":"Single-phase bridge rectifier: Example of the application of the graphical symbol in a diagram","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11385,"name":"Three-phase bridge rectifier","lib_id":524,"cn":"Three-phase bridge rectifier","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11386,"name":"Diode matrix (fragment)","lib_id":524,"cn":"Diode matrix (fragment)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11387,"name":"Diode matrix: If all diodes in the matrix nodes are connected identically, a simplified method of depiction is permitted","lib_id":524,"cn":"Diode matrix: If all diodes in the matrix nodes are connected identically, a simplified method of depiction is permitted","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11388,"name":"Diode","lib_id":524,"cn":"Diode","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11389,"name":"NPN transistor","lib_id":524,"cn":"NPN transistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11390,"name":"PNIP transistor (I-region lead)","lib_id":524,"cn":"PNIP transistor (I-region lead)","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11391,"name":"Diode thyristor","lib_id":524,"cn":"Diode thyristor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11392,"name":"Triode thyristor","lib_id":524,"cn":"Triode thyristor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11393,"name":"Transistor","lib_id":524,"cn":"Transistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11394,"name":"Field-effect transistor","lib_id":524,"cn":"Field-effect transistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""},{"id":11395,"name":"Insulated-gate field-effect transistor","lib_id":524,"cn":"Insulated-gate field-effect transistor","en":"","jp":"","de":"","fr":"","es":"","ru":"","it":"","pt":"","kr":"","tw":"","name_id":""}],"msg":""}